3. CUSTOMIZING YOUR NOTETAKER
3.1 Set Time and Date
3.2 Setup Internet
3.2.1 Setup Wireless LAN
3.2.2 Modem & Bluetooth DUN setup
3.2.3 Advanced Settings.
3.3 Bluetooth Manager
3.3.1 Bluetooth Device List
3.3.2 Bluetooth Service List
3.4 Pronunciation Dictionary
3.5 Menu manager
3.6 Backup/Restore Personalized settings
3.7 Change device Name
3.8 Password Protection
3.8.1 Setting and modifying passwords.
3.8.2 Password Configuration
3.8.3 Reset Password to factory defaults.
3.9 Global Options
3.9.1 Global Options Overview
3.9.2 Global Options in Detail

3. Customizing your Notetaker
When you receive your notetaker, one of the first things you will want to do is to configure it to act the way you want it to. The "Settings" menu on the U2 allows you to configure and customize your notetaker to meet your specific needs and preferences. 
To open the "Settings" menu, press "F1" to bring up the main menu. Press "Space-4" until you reach "Settings" and press "Enter". Or, just press S from the main menu to quickly jump to and open the "Settings" menu.
The "Settings" menu contains 9 items: "Set Time and Date", "Setup Internet", "Bluetooth Manager", "Pronunciation Dictionary", "Menu Manager", "Backup/Restore Personalized Settings", "Change Device Name", "Password Protection" and "Global Options". The following sections discuss each of these items in detail.

3.1 Set Time and Date
To set the U2's internal clock, press "Enter" on "Set Time and Date" in the "Settings" menu.  Or press T to open the "set time and date" dialog from the menu. You can launch the "Set Time and Date" dialog from anywhere on the unit by pressing "F3-T". 
The set time and date is a dialog, consisting of the following: "Time zone", "Use Daylight Savings", "Time format", "Time", "Date Format", "Date", "Synchronize with time server", a "Confirm" button, and a "Cancel" button. You can move among these items by pressing "tab (Space-4-5)" or "shift-tab #Space-1-2)".
When you activate "Set Time and Date" for the first time, "Time zone?" appears followed by the default time zone.  You can choose your desired time zone by navigating to it using "Space-1" or "Space-4" or by typing the first letter of the time zone. Select your time zone, and move to the next item by pressing "F3".
The "Use Daylight Saving" check box displays only if it is used in the current "Time zone".  You can check and uncheck this item using "Space".
The next item is "Time format", the options for which are 12 hour and 24 hour time. You can toggle between the two using "Space-1" or "Space-4". 
The next item is "Time". Use this option to set the clock's time. If you select 12 hour clock in the "Time format", A.M. or P.M. is displayed after the hour and minute. In the 12 hour clock, you can toggle A.M. it P.M. by pressing "Space-X".  When typing the time, separate the hour and minute using a space or a colon. 
Tab to "Date format". You can choose to display the date in either the "short" or "long" format. The short format displays the date numerically, while the long format displays the Month spelled out and shows the date as it would appear in literary form. Toggle between the two using "Space-1" and "Space-4". 
The next item is "Date". Type the "Date" month, date, and year  as mm/dd/yyyy. Use 2 digits for the month, 2 digits for the day, and 4 digits for the year, separating them by a space or a slash. 
The next item is "Synchronize with time server", used to synchronize time and date with a time server on the Internet. This function is extremely useful when the date and time of U2 is faster or slower than the current time. To execute this function, your U2 must be connected to the Internet. When connected, press "Enter" on the "Synchronize with time server" button. After synchronization, it displays the synchronized time in the "Time" edit combo box. The synchronized date is also displayed in the "Date" edit combo box.
If you do not wish to enter date and time information directly, you can navigate using the following commands:
When setting time:
Move forward 1 hour: Space-4
Move back 1 hour: Space-1
Move forward 10 minutes: Space-5
Move back 10 minutes: Space-2
Move forward 1 minute: Space-6
Move back 1 minute: Space-3
When setting date:
Move to the next day: Space-6
Move to the previous day: Space-3
Move to the next week: Space-5
Move to the previous week: Space-2
Move to the next month: Space-4
Move to the previous month: Space-1
Move to the next year: Space-5-6
Move to the previous year: Space-2-3

When you have completed entering all of the information, press "Enter" to save your settings, or "Tab to "Confirm" and press "Enter", and you are returned to the "Settings" menu.

3.2 Setup Internet
The "Setup internet" function is used to configure your U2 to use various connection types to access the Internet. The "Setup internet" utility contains the following connection options: "Wireless LAN", "Modem", and "Bluetooth DUN". You can move among the items by pressing "Space-4" or "Space-1". To connect to the Internet via a wireless network, use the "Wireless LAN" option. The "Modem" setup should be used if you are connecting to the Internet via a broadband  modem. 
To activate "Setup internet", press "Enter" on "Setup internet" in the "Settings" menu, or press "I". You can open the "Setup Internet" menu from anywhere on the unit by pressing "F3-I". 
Or, if the PC on which the Active Sync program is installed is connected to the Internet, and the U2 is connected to that PC, you can also connect the U2 to the Internet via that connection.
The various connection types are explained in greater detail in the following sections.

3.2.1 Setup Wireless LAN
Before setting up a Wireless LAN connection, be sure wireless is turned on in the "Global Options" dialog. You can toggle wireless on and off from anywhere on the U2 using "Backspace-1-4-5-6". In addition, when you choose this option, if Wireless is not turned on, Braille Sense automatically activates Wireless LAN. To connect to a wireless network, navigate to the "Wireless LAN" option in the connection types list under "Setup Internet" and press "Enter". 
The "Wireless LAN" dialog consists of the "access points" list, "Advanced" button and "Close" button. You can move among these controls by pressing "F3" or "Space-F3". If wireless is not turned on, the "access points" list displays "no items". 
When wireless is on, this list shows the wireless "access points" (networks) in range of your notetaker. The "Access points" list displays the "access point name", "encryption", and "sensitivity" of each item. (Ex: linksys, encryption: WEP, sensitivity: good.) If there is more than one access point in the list, you can move among them by pressing "Space-1" or "Space-4". Move to the "access point" to which you want to connect, and press "Enter". If the access point has no encryption, the U2 announces, "Connecting to (access point name)". If connection is successful, the connecting sound is heard. If the network is encrypted and requires a network key, when you press "Enter" on the access point, the "Network key" edit box is displayed. Type the network key in computer Braille in the edit box and press "Enter". If your settings are correct, the unit says, "Completed setting profile" and the connecting sound is heard. 
The "Advanced" dialog is used to modify an existing profile, manually add a new profile, or check the settings of an existing profile. If you press "Enter" on the "Advanced" button while wireless LAN is turned off, "no items" is displayed. Pressing "Enter" on the "advanced" button, while wireless LAN is turned on, displays a list of the wireless profiles saved on the U2.
The "Advanced" dialog has 5 controls: the "profile list", "Connect" button, "Add" common dialog button, "Remove" button, "Properties" common dialog button, and "Close" button. You can navigate among these controls by pressing "F3" or "Space-F3". Navigate the items in the Profile list using "Space-1" and "space-4". Press "Enter" to activate one of the buttons.
Use the "Add" button: to manually add a profile, specifically where an SSID is hidden, and thus does not appear in the "access points" list. The "Add" dialog" contains 10 controls.
1) "Setup IP: Automatic" combo box: You can switch between automatic and manual by pressing "Space-4" or "Space-1". If you select "Manual", you must enter your IP address, subnet mask, gateway IP address, and DNS IP address. You can move among these computer edit boxes by pressing "Space-4" or "Space-1". Press "tab (Space-4-5)" to move to the next control.
2) "Network name (SSID)" computer edit box: Type the network ID in the computer edit box.
3) "Network mode" combo box: You can select among "Infrastructure", and "802.11 ad-hoc" mode by pressing "Space-1" or "Space-4".
4) "Network authentication mode" combo box: Select among "Open", "Shared", "WPA-PSK", and "WPA2-PSK" by pressing "Space-1" or "Space-4".
5) "Data encryption" combo box: Select the data encryption method by pressing "Space-1" or "Space-4". If you select "Open" or "Shared" in network authentication mode, you can choose among "Disable" and "WEP". And if you select "WPA-PSK" or "WPA2-PSK" in network authentication mode, either "AES" or "TKIP" can be selected in the "Data encryption" combo box.
6) "The key is provided automatically" check box: If the "access point" does not provide a key for users automatically, uncheck this check box by pressing "Space". The default is checked. 
7) "Network key" computer edit box: This is a computer edit box to type the network key if the key is not provided automatically.
8) "Key index" edit box: This is an edit box to type the key number of the wireless access point that matches the network key input.
9) "Confirm" button: Pressing this button applies the changes.
10) "Cancel" button: You can select this button to cancel the setup.
* Things to note: 
1) If "Data encryption" has been set as "disabled", press "F3" and you are taken directly to the "Confirm" button. 
2) "Network key" and "Key index" is displayed only if you uncheck "The key is provided automatically".

To delete a profile item in the profile list, select the profile item you wish to delete, and press R or "Tab" to the "Remove" button and press "Enter". 
To get information about a selected profile item in the profile list, "Tab" to the "Properties" button and press "Enter". In the "Properties" dialog, you can reconfirm or modify the information for each profile. 
To exit the "Advance" dialog, press "Space-E" or "Space-Z".

3.2.2 Modem & Bluetooth DUN setup
Before setting up the U2 to connect to the Internet via a modem, you must connect a USB 3G modem card to the USB port. From the list of connection types under the "Setup internet" option in the "Utilities" menu, move to the modem by pressing "Space-1" or "Space-4," and press "Enter." 
If you wish to connect to a Mobile network using Bluetooth DUN, move to "Bluetooth DUN" and press "Enter". Bluetooth DUN does not require the insertion of a modem, however, its user interface is the same as setting up a connection using the modem.
The modem setup contains the following: "connect list", "Default", "Add", "Modify", "Delete", and "Close". You can move among these controls by pressing "F3" or "Space-F3". You can move among the items in each control by pressing "Space-4" or "Space-1".
The "connect list" contains previously added connection configurations. You can move among these by pressing "Space-4" or "Space-1".
The "Default" is to set the default connection to use when connecting via a modem. To set a connection as the default, move to the "connect list", and navigate to "Default" by pressing "F3" and press "Enter".
"Add" is a dialog for creating a modem connection configuration. It contains "connection settings list", a "Confirm" button, and a "Cancel" button.  The "connection settings list" contains "Connect name", "Connect number", "ID", "Password", and "Modem speed". In the "Connect name" edit box, type the host name or something that clearly identifies this connection to you. In the "Connect number" edit box, type the number of the host in computer Braille. 
* Note: you can type numbers and commas only. If the connection requires an ID and password, enter these in the appropriate edit boxes using computer Braille. If the connection does not require an ID and password, leave these blank. In the "Modem speed", combo box, select one from the list by pressing "Backspace" or "Space". When you have entered all of the necessary information, press "Enter" to save the connection configuration. To cancel creation of the connection, Tab to "Cancel" and press "Enter" on it.
"Modify" is used to change the information in a given connection configuration. To do this move to the connection you want to modify and press "Enter". You can also "Tab" to "Modify" and press "Enter". Or, you can press "Enter-M on the "Connect name" in the "connect list". "Modify" contains the same items as the "Add" dialog, and you navigate and set the values in the same way.
To delete an item, move to the connection you want to delete, and press "Enter" on the "delete" button.  Or, you can delete an item by pressing "Space-D" on the connection you wish to delete. 
To exit the "Modem setup", press "Space-Z" or "Tab" to the "Close" button and press "Enter". 

3.2.3 Advanced Settings.
The "Advanced Settings" item allows you to set up the use of an auto configuration script and/or a proxy server. 
To use an auto configuration script, Open the "Advanced Settings" dialog, and press "Space" on the auto Configuration Script" check box to check it. When you check this item, a computer edit box appears in to which you should type the address for the auto configuration script you wish to use. Tab to the "Confirm' button, and press "Enter to save your settings.
To use a proxy Server, Open the "Advanced Settings' dialog, and press "Space" on the "Use Proxy Server" check box. Other items appear for configuration of the proxy server setup. The first is a checkbox to toggle whether to "bypass for local addresses". Press "Space" to toggle this on or off. Tab to the "Proxy server address" computer edit box, and type the address of your proxy server.
Tab to the "Confirm" button and "Press 'Enter" to save your settings, or Tab to the "Cancel" button and press "Enter" to cancel the "Advanced Settings" dialog. 

3.3 Bluetooth Manager
The U2 is Bluetooth capable, or rather, you can connect the U2 to various devices such as keyboards, printers, audio devices, and other computers without the need for cables. You can also use Bluetooth to transfer files, or to connect the U2 as a Braille display with a compatible screen reader. Bluetooth is the latest in wireless technology and enables wireless connectivity via a Personal Area Network (PAN). Unlike a traditional Wireless Local Area Network (WLAN), these networks are limited to approximately 30 feet or less. Bluetooth enables users to exchange various types of information over this wireless connection. 
You can toggle Bluetooth on/off from anywhere on the unit using "Backspace-dots-3-4-5-6". If you do not activate Bluetooth before opening the Bluetooth Manager, Braille Sense automatically activates it. 
To access the Bluetooth Manager from the program menu, navigate to the "Settings" menu, and press "Enter. Then, navigate to "Bluetooth Manager", and press "Enter". You can  also press "F3-B" to launch the Bluetooth Manager from anywhere on the unit.

3.3.1 Bluetooth Device List
When the Bluetooth Manager is activated, it begins scanning for other Bluetooth devices that are in range, and the services available from the other Bluetooth devices. For example, if you have a computer with Bluetooth enabled nearby, the U2 attempts to find it. It may take 30 to 40 seconds to discover all of the Bluetooth devices in range. The U2 announces and displays, "Scanning for devices. Please wait...". Progress beeps are heard during the scanning process, and full cells are filled in on the Braille display to indicate scanning progress. 
When a Bluetooth device is detected, the U2 announces "found (Bluetooth device name)". 
* Note: while the U2 is scanning for Bluetooth devices, it cannot respond to key presses. In addition, you may not cancel the scan once it has begun, but must wait for its completion before the U2 returns to normal operation.  
When the scanning process completes, you are placed in the Bluetooth Device List. If the U2 has found other Bluetooth devices in range, they are displayed as "device name (untrusted (or trusted)) xx/yy" where xx is the number at which the device appears in the list, and yy is the total number of devices. "Trusted" indicates that the service has been authenticated, "untrusted" indicates the service has not been authenticated.
If there are no other Bluetooth devices in range, the U2 announces, "no items". You can press "Space-1" or "Space-4" to move through the list. To select a device from the list, press "Enter" on the device name.
If the Bluetooth device is trusted, settings for connecting the device are automatically saved in the U2. If you want to delete this information, press "Space-D" on the Bluetooth device name in the list. The U2 announces, "Device settings removed". Removal of the settings applies only to the current device.
From the Bluetooth Device List, you can access the menu by pressing "F2". The "Bluetooth Device List menu" contains "Rescan For Devices", "Device Name", "Delete Pair Information", and "Exit". You can navigate among the menu items using "Space-1" or "Space-4".
The first menu item is "Rescan For Device". This option initiates a new scan for other Bluetooth devices. To activate this item, press "Enter" on "Rescan For Devices" in the menu.  Or you can activate it directly from the list by pressing "Enter-R". 
 To activate the "Device Name" function, navigate to it in the menu and press "Enter". You can access it directly from the device list by pressing "Enter-N". 
This item allows you to specify the device name given to the U2. The default name for the Bluetooth device name is "BrailleSenseU2".  When you activate this option, you are placed in a computer edit box that contains your current device name. To modify the name, type the new name and press "Enter". After entering the new name, you should close all programs and reset the U2 by pressing the "Reset" button on the rear panel of the unit. To cancel your changes, press "Space-E". You are returned to the Bluetooth Device List.
The next menu item is "Delete Pair Information". This item allows you to remove the connection settings for the current device. To activate this item, press "Enter" on "Delete Pair Information" from the menu, or press  "Space-D" to activate it from the Device List. 
The final item in the Bluetooth Device List menu is "Exit". This option exits the Bluetooth Manager program. To activate this item, press "Enter" on "Exit" from within the menu, or exit the program any time by pressing "Space-Z". 

3.3.2 Bluetooth Service List
When you locate a Bluetooth device to which you'd like to connect, press "Space-1" or "Space-4" to navigate to the device in the Bluetooth Device List, and press "Enter" on the device name. The unit announces, "Scanning for services. Please wait...". Please note The U2 does not respond to key presses during the scanning process. 
The U2 supports the following Bluetooth services: LAN, FTP, ActiveSync, Serial port, USB port, headset, and Bluetooth DUN. To access any of these functions, be sure that the remote Bluetooth device is in Discoverable mode, and that the service you wish to access is enabled on that device. It is possible to have certain services enabled on your remote Bluetooth device, while disabling others. For example, you could have LAN and FTP enabled, while having ActiveSync and Serial Port disabled. The U2 only sees and displays services which are enabled on your remote device, even if others are available. 
When the U2 has found all of the available services, the services are displayed in a list in the following format: "service name xx/yy" where xx is the number at which the service appears in the list, and yy is the total number of available services. You can move through the available services by pressing "Space-1" or "Space-4". Press "Backspace" to return to the Bluetooth Device List.
From the Bluetooth Service List, you can access the menu by pressing "Space-M" or by pressing "F2". The "Bluetooth Service List menu" contains "Device Name", "Open FTP", "Disconnect" and "Exit". You can navigate the menu items using "Space-1" or "Space-4".
The "Device Name" and "Exit" options in the "Bluetooth Service List" menu are the same as those in the "Bluetooth Device List" menu. 
The "Open FTP" menu item allows you to quickly open a direct FTP connection with a remote Bluetooth device without accessing the Device and Service lists. However, you must have connected the FTP service previously for the U2 to allow you to transfer files. If you have not connected the FTP service, and you activate this function, the unit announces, "FTP service disconnected". 
You can access "Open FTP"  by pressing "Enter" on it from within the menu, or by pressing "Enter-T" directly from the Bluetooth Service List.. The U2 says, "Connecting service". Detailed information on connecting various service types is covered later in this chapter.
The "Disconnect" menu item allows you to disconnect services with other Bluetooth devices. You can access this item by pressing "Enter" on "disconnect" from within the menu. Or you can activate it directly from the Bluetooth Service List by pressing "Enter-D". 
If there are no services connected and you activate this function, the unit says, "There is no service connected".

3.3.2.1 Connecting  a Service
To authenticate a service and connect to it, press "Enter" on the service. The U2 announces, "Connecting service". You are then prompted for a "PIN code:" You must use ASCII characters when you type the pin code. This edit box only appears when you have not previously connected to a service, and a pin code is required by the device. You can exit the edit box or delete text you have typed by pressing "Space-Z" and you are returned to the Bluetooth Service List.
When you finish typing the pin code, press "Enter". The unit announces, "Please wait for authentication". If the remote device is setup correctly, and has not been set up to allow this device to always connect, the remote device also asks for a pin code. Please be sure to enter the same pin code on both devices. If the remote Bluetooth device pin code matches the pin code on the U2, the service should authenticate. If connection is successful, the unit announces, "PIN code authentication accepted". 
You are then prompted, "Please wait. Access permission". If the remote Bluetooth device does not give access permission, the unit says, "Connection failed", and you are returned to the Bluetooth Services List. If the remote Bluetooth device gives you access permission, the U2 says "Connection succeeded". If the connection succeeds, "Connected" is displayed after the service in the Bluetooth Service List. Some services may be connected without inputting a pin code depending on the Remote Bluetooth device settings.

3.3.2.2 LAN Service
You can use the LAN service to access the Internet via your computer's Internet connection. If you connect this service, you can use the Web browser and email program, as if you were connected to the Internet via Ethernet or wireless LAN. Before you can connect to the LAN service on a remote Bluetooth device, the device must be configured for Internet Connection Sharing (ICS). If ICS is not properly setup, you cannot connect to the Internet using the LAN service. For information on how to setup ICS for your remote Bluetooth device, please refer to the documentation that came with your Bluetooth adapter. Setting up ICS requires knowledge of network architecture, so it may be a good idea to contact a local network technician or your network administrator for help with setting up ICS.

3.3.2.3 FTP Service
This service works similarly to using FTP on the Internet. It allows you to transfer folders and files to and from the remote Bluetooth device. When referring to the FTP service, we will refer to the file/folder list on the remote Bluetooth device as the "remote folder list" and the file/folder list on the U2 as the "local folder list".
After you have successfully connected to the FTP service, the Bluetooth Manager places you in the remote folder list. The remote folder list displayed is determined by the remote Bluetooth device. Typically, this folder is called the Bluetooth Exchange Folder, but you should check your remote Bluetooth device documentation for definitive information. 
You can interact with the remote folder list in much the same way as you interact with files and folders in the File Manager. With the FTP service, you can perform the following functions: Copy, Paste, Send To, Retrieve File, New Folder, Delete File/Folder, Open Local Folder, Select All and Information.
If you press "Enter" on "Local Folder", you are taken to the local folder list. If you are in the local folder list, this menu option changes to "Move to remote folder". In the next few sections, we will discuss the various FTP functions. Please note that while sending data to and from the remote Bluetooth device, the remote Bluetooth device may still need to give access permission to the U2. Please consult the documentation for the remote Bluetooth device for details.

3.3.2.3.1 Copy and Paste
These functions allow you to copy and paste files between the local folder and the remote folder.
Use the following steps to copy files from a local folder to the remote folder:
1) From the remote folder list, press "F2" to open the FTP menu. Press "Space-1" or "Space-4" to navigate to "Open Local Folder", and press "Enter".  Press "Enter-o (dots 1-3-5)" to open the local folder directly from the remote folder list. The unit says, "Opening Local Folder", and you are placed in the Disk list that appears in File Manager. You are placed on "flashdisk" by default, but if you have an SD card or USB memory stick inserted, you can navigate to them by pressing "Space-1" or "Space-4".
See section 4 of this manual for more information on navigating files and folders. 
2) As when navigating in the File Manager, you can access a disk by pressing "Enter" on it. Use the same navigation keys as in the File Manager to navigate the local folder. Note that you cannot select folders. You can only select files. If you try to select a folder, the U2 says, "Deactivated".
3) Once you have selected files by pressing "Space", you can copy them by pressing "Enter-C" 
4) U2 announces, "Copying" and "Open Remote Folder". You are then returned to the remote folder list.
5) In the remote folder list, navigate to the folder where you want to paste the file. Press "Enter-V". Or, you can press "Enter" on "Paste" from the menu. If the file is larger than 300 KB, progress messages are spoken each time an additional 10% is completed. If the file is less than 300 KB, only progress beeps are heard. 
6) When the file is pasted successfully, the U2 displays the message, "xxx file pasted", where xxx is the name of the file. If the file is not pasted successfully, "xxx file not pasted" is displayed. After the file is pasted successfully, the unit also announces, "Paste completed", and you are returned to the remote folder list.
You can use the same procedure to copy files from the remote folder to the local folder.

3.3.2.3.2 Send To
This function allows you to send files from the local folder list to the remote folder list. 
* Note: this option is only available in the local folder list. This is very similar to the copy and paste function with a couple of notable differences. One difference is that you do not have to paste the file to the remote folder. It is done as soon as you activate the "Send To" function. ANOTHER difference is that when you activate this function, the file can only be sent to the root of the remote folder list. To copy a file using the "Send To" function, follow these steps:
1) From the "remote folder list", press "Enter-O" to open the local folder.
2) Select a file by navigating to it and pressing "Space". 
* Note: you can select only files; folders cannot be selected.
3) After you have selected a file, press "Enter" on "Send To" from within the menu. Or, press "Enter-S" to activate the "Send To" function directly.
4) When the transfer is complete, the unit announces, "xxx file sent", where xxx is the name of the file. If the file does not transfer, the unit says, "xxx file not sent". When all selected files are transferred, the U2 announces, "Successfully sent", and you are returned to the remote folder list.

3.3.2.3.3 Retrieve File
The "Retrieve File" function allows you to retrieve a file from the remote folder list, and move it to the local folder. This function is only available from the remote folder list. When using this function, all retrieved files are saved to the "flashdisk/download" folder. Use the following steps to retrieve a file: 
1) Navigate the remote folder list using normal file and folder navigation.
2) Press "Space" to select the file you want to retrieve. Note that you can select only files, not folders.
3) After selecting the file, press "Enter" on "Retrieve File" from within the menu, or activate it directly by pressing "Enter-R". 
4) As with copying and pasting, progress beeps are heard.  When the transfer is complete, the unit announces, "xxx file retrieved", where xxx is the name of the file. If the file does not transfer, U2 says, "xxx file not retrieved". When all of the selected files are transferred, the message "Retrieve completed" is spoken, and you are returned to the remote folder list.

3.3.2.3.4 New Folder
The "New Folder" function allows you to create a new folder in either the local folder list or the remote folder list. Use the following steps to create a new folder: 
1) With the FTP service connected, from either the local or remote folder list, navigate to the folder in which you want to create a new folder. Move between the "remote folder list" and "local folder list" by pressing "Enter-o (dots 1-3-5)".  
2) Select "New Folder" from the menu. Or, activate "New Folder" directly from the folder list by pressing "Enter-F". 
3) An edit box appears and the unit prompts, "New folder name:". Type the new folder name using ASCII characters, and press "Enter". If the folder is created successfully, the U2 says, "xxx folder created", where xxx is the name of the folder. You are then returned to your previous location. 
4) To cancel the folder creation, press "Space-Z" and you are returned to the previous list.

3.3.2.3.5 Delete File/Folder
Note that if a folder contains sub-folders, you cannot delete the folder. To delete a file or folder from the remote or local folder, do the following: 
1) Navigate to the local or remote folder list, and select the items you want to delete. 
2) Press "Enter" on "Delete File/Folder" from the menu, or press "Space-D" directly from the folder list.
3) If the items are deleted successfully, "Delete completed" is spoken.

3.3.2.3.6 Information
This function allows you to obtain information about files or folders located in the remote or local folder list. follow these steps:
1) Navigate to the local or remote folder list, and select the file or folder about which you want information. 
2) Select "Information" from the menu, or, from the folder list, press "Enter-I". 
3) The "Information dialog box" appears. The dialog box contains "Type", "Size", "Date", "Attribute (except for folders)", and "Close". Move among these controls by pressing "F3" or "Space-F3". If you select multiple files, the "Information" dialog displays the number of selected files and total size.

3.3.2.4 ActiveSync Service
This service offers the same functionality as connecting the U2 to a computer via USB and using ActiveSync. If the connection to the ActiveSync service is successful, you will hear the chime indicating ActiveSync is successfully connected. As with all of the Bluetooth services, the remote Bluetooth device may need to authorize the U2. You are then returned to the Bluetooth Service list. As with using ActiveSync via USB, you can copy and paste files from the U2 from the remote Bluetooth device to the U2 and vice versa.
You cannot use ActiveSync via USB and Bluetooth at the same time. If the remote Bluetooth device is connected via USB and using ActiveSync, you must terminate the USB ActiveSync connection on the remote Bluetooth device in order to use the ActiveSync service via Bluetooth.

3.3.2.5 Serial Port
If you connect this service, you should not connect to other Bluetooth services. The Serial Port service allows you to use your U2 as a wireless Braille display via Bluetooth. 
* Note: you must be using a compatible screen reader to use the U2 as a wireless Braille display. See section 13.7 for information on connecting and using U2 with various screen readers.   

3.3.2.6 Bluetooth keyboard service
Before you try to use this service, please be sure the Bluetooth keyboard is turned on and in Bluetooth range.
Use the following steps to connect to a Bluetooth keyboard:
1) Navigate to the Bluetooth keyboard  in the Bluetooth Device List and press "Enter". 
2) "Keyboard" should be displayed in the list of available services. 
3) Press "Enter" on the "Keyboard" service.
4) If the keyboard requires a PIN code you are prompted to enter it. Some devices do not require a PIN code, in which case, you are not prompted to enter one. 
5) If you are prompted, input the  PIN code on the U2 and press "Enter". If the keyboard requires a PIN code, you must also input the PIN code on the Bluetooth Keyboard. (You should be able to locate PIN code information for the Bluetooth keyboard in the documentation that came with it.)

3.3.2.7 Bluetooth Printer service
Follow these steps to connect to a Bluetooth enabled printer:
1) Press "Space-1" or "Space-4" to navigate to the Bluetooth enabled printer in the Bluetooth Devices List and press "Enter".
2) The U2 scans for available services.
3) Press "Space-1" or "Space-4" to navigate to the "Printer" service and press "Enter0..
4) The printer should connect to U2.

3.3.2.8 Using Multiple Services 
You can use the LAN, FTP, and ActiveSync Bluetooth services simultaneously. However, if you plan to use any of these services at the same time, you should connect the FTP service before connecting the LAN and ActiveSync services. If you do not connect the FTP service first, you may experience problems. If you are using the Serial 
Port service, you should not connect to any other Bluetooth services.

3.4 Pronunciation Dictionary
The "Pronunciation dictionary" is used to modify how U2 pronounces specified words as defined by your entries into the dictionary.  You can open it by pressing P from the "Settings" menu. You can also launch the "Pronunciation Dictionary" from anywhere on the unit by pressing "F3-P". 
The "Pronunciation dictionary" is composed of the list, "Add Word" button, "Modify Word" button, "Delete Word" button and "Close" button. You can move among these controls by pressing "F3" and "Space-F3".
The list is shown as "word: xx "yy" where "xx" is the original word and "yy" is the alternative pronunciation. For example, if you wanted to hear "Who" pronounced as "world health organization" and you added the word to the pronunciation dictionary, it is listed as "word: WHO "world health organization". You can move up or down through items in the pronunciation dictionary by pressing "Space-1" or "Space-4". You can also click the cursor routing key corresponding to the item position you want to focus. For example, if there are 10 items in the list and you want to focus the 5th item, you can click the 5th cursor routing key and your focus is placed on the 5th item on the list. The pronunciation dictionary does not list entries in alphabetical order, but rather, in the order they were added to the dictionary. 
To add a new word, press "Enter" on the "Add Word" button or you can press "Space-I". You are prompted to, "Add entry:" Type the word for which you want to change the pronunciation and "Tab" to "Replacement:" Type the letters that produce the alternative pronunciation you desire. Press "Enter" or "Tab" to the "Confirm" button and press "Enter". The word is added, and the focus is returned to the "Add Word" button.  To cancel this modification, press "Enter" on the "Cancel" button or press "Space-E" or "Space-Z". 
To modify a stored entry, navigate to the item you want to modify. "Tab" to the "Modify Word" button and press "Enter". Or when the entry is focused, press "Space-M". You are prompted to, "Modify entry: (focused word)". Press "F3" and you are placed in the "Replacement: (new pronunciation)" edit box. Type the new replacement pronunciation text and press "Enter". Or "Tab" to the "Confirm" button and press "Enter". The word is modified and the focus is returned to the "Modify Word" button. To cancel this modification, press "Enter" on the "Cancel" button or press "Space-E" or "Space-Z". 
To delete a stored entry, navigate to the entry you want to delete. "Tab" to the "Delete word" button and press "Enter". Or, press "Space-D" on the item you want to delete. You are prompted, "Delete? Yes". To delete the item, press "Enter". To abort deletion, press "Space" to change to "No" and press "Enter".
To exit the "Pronunciation dictionary", press "Enter" on the "Close" button or press "Space-Z".

3.5 Menu manager
Using the Menu manager on the U2, you can manage what menus and/or programs are displayed in the Main Menu or sub menus. You can show or hide almost any program in the Main Menu with a few exceptions. You may not hide the File manager, the Menu Manager itself, or the "Programs" menu which only appears if external programs are installed. 
To execute the "Menu manager", from the "program" menu, press S" to open the "Settings"" menu. Press M to open "Menu manager". The "Menu manager'" dialog is displayed. You can also launch the "Menu Manager" from anywhere on the unit by pressing "F3-M". 
The dialog of the "Menu manager" consists of the following items: The menu/program list, "Modify Menu Name" button (Only appears when cursor is placed on a menu), Confirm button and Cancel button. To navigate among the programs, press "Space-1" or "Space-4". Press "F3" or "Space-F3" to navigate to the "Confirm" and "Cancel" buttons. 
When placed on a menu such as "Media" or "Web Tools", you do not have the option of showing or hiding the item. Menus are displayed if they have programs accessible inside them. If you have chosen to hide all the programs in a given menu, this menu is not displayed. 
When your cursor is placed on a menu, you have the option of renaming the item. To rename a menu item, navigate to the menu you wish to rename. "Tab" to "Modify Menu Name", and press "Enter". Braille Sense prompts, "Menu Name", and you are placed in an edit box in to which you can type the new menu name. When you have typed the new name in to the edit box, press "Enter", or tab to "Confirm" and press "Enter". 
To hide unused programs on the U2, press "Space" on each of the programs you wish to hide in the list. Press "Enter" to save your settings, or tab to "Confirm" and press "Enter". You must reset the U2 using the "Reset" button on the back of the unit for these settings to take effect. When the U2 reboots, the programs you chose to hide are no longer displayed. 
To unhide the programs, return to the "Menu Manager" dialog, and press "Space" on the programs you wish to unhide, and press "Enter" to save the settings. Press "Reset" once again, and the programs reappear in the menus after the unit reboots. 

3.6 Backup/Restore Personalized settings
If you hard reset your U2, or its battery is fully discharged, the main option settings and settings for each program are initialized to the default values. If you have created a backup of your settings, you can restore the option settings after the hard reset.
"Backup/Restore Personalized settings" is a utility used to backup/restore the option settings for each program in the U2 all at once. You can run this utility by pressing K from the "Settings" menu.  You can also launch the "Backup/Restore Personalized Settings" dialog from anywhere on the unit by pressing "F3-K". 
The "backup/restore" dialog contains: the "program option check box list", a "Select all" button, a "Backup" button, a "Restore" button, and a "Cancel" button. You can move among the check boxes in the "program option check box list", by pressing "Space-1" or "Space-4". You can move among the controls in the dialog by pressing "F3" or "Space-F3".
The "program option check box list" contains "Options settings", "File manager options", "Word processor options", "Address manager options", "Schedule manager options", "Media player options", "Web browser options", "E-mail options", "DAISY Player options", "Radio options", "Bluetooth manager options", "Social Networking options", "Database manager options" and "BookShare Download options".
In this list, move to the program options you want to backup or restore and check the item by pressing "Space". You can uncheck a checked item by pressing "Space" again. To select all of the program options in the list, press "Enter" on the "Select all" button. 
After selecting all the options you want to backup or restore, press "Enter" on the "Backup" or "Restore" button, or press "Enter-B" to backup or "Enter-R" to restore. If you select the "Backup" button, you are prompted to select a path for storing the backup file. Navigate to the folder in which to store the backup files using normal file/folder navigation commands. Select the folder or drive in which to store the backup by pressing "Space", and press "Enter" to start the backup process. Each of these options has its own backup file. This means that if you backup options for 5 programs, the utility generates 5 backup files. 
If you select the "Restore" button, you are prompted for the path from which to restore backup files. Again, use normal file and folder navigation to select the folder containing your backup files. If you select a folder in which there is no backup, you receive a message indicating there is no backup option file. To restore your settings, select the folder containing the backup files by pressing "Space", then press "Enter" to initiate the restore process.

3.7 Change device Name
The "Change device Name" function allows you to change the Bluetooth/network name of your unit. By default, the Braille Sense is named something like "U2035". You may wish to give it a more personalized name in order to identify it more easily when pairing with another device. This is especially important when using "Sense Chat" as you'll be pairing 2 Sense notetakers, and it is important to know which is which. 
You can access the "Change device Name" dialog by navigating to the "Settings" menu, then to "Change Device Name". You can also launch the "Change device Name" dialog from anywhere on the unit by pressing "Backspace-Enter-E". 
The "Change device Name' dialog consists of 3 controls: a "Device Name" edit box, a "Confirm" button, and a "Cancel" button. Use "F3" and "Space-F3" to move among the controls.
To change your device name, type a new name in the edit box and press "Enter". Or, after typing the new name, tab to "confirm" and press "Enter". If you decide you do not wish to change your device name, tab to the "Cancel" button and press "Enter", or press "Space-E" or "Space-Z".
Once you have changed your device name, it is necessary to reset the unit for the change to take effect. Reset the unit by pressing the small round button on the back. The next time you use another device to search for Bluetooth devices, your Braille Sense should appear under your new name.

3.8 Password Protection
The Password Protection item allows you to set a password that must be entered when the unit is powered on, comes out of Sleep Mode, is upgraded, or the disk is formatted.
To open the "Password Protection" settings, from the Main menu, navigate to "Settings" and press "Enter".  Press A to jump to and open "Password Protection". You can open "Password Protection" from anywhere on the unit by pressing "F3-N". 
The "Password Protection" dialog consists of 4 items: "set/modify Password" dialog, "Password Configuration" dialog, "Set Password to factory defaults", and a "Close" button. Use "F3" or "Space-F3"  to move among the controls in the dialog.

3.8.1 Setting and modifying passwords.
When you open the "Password Protection" program, you are placed on the "Set Password" option. Press "Enter" to open the "Set Password" dialog. The "Set Password" dialog consists of 4 controls: "Password" edit box, "Retype Password" edit box, "Confirm" button and a "Cancel" button". 
Type the password you wish to use into the "Password" edit box. Tab to the "Re-type Password" edit box, and type it again. To save the password, press "Enter", or Tab to "Confirm" and press "Enter". To cancel saving the password, press "Space-Z", or Tab to the "Cancel" button and press "Enter".
When a password is saved, the "Set Password" option is replaced with "Modify Password". Once you have entered a password, you can modify in very much the same manner. The "Modify Password" dialog consists of all the same controls, except you must type your current password, before you can type a new one. Once you have typed your current password, then the new password, you must re-type the new password. Press "Enter" on the "Confirm" button to save the new password, or "Enter" on the "Cancel" button to cancel the modification.

3.8.2 Password Configuration
The "Password Configuration" dialog allows you to define when you are prompted to enter the password. When you press "Enter" to open the "Password Configuration" dialog, you are prompted to enter your password to gain access to this configuration. Type your password, and press "Enter".
The password configuration settings consist of 4 radio buttons: "Prompt for password on boot", "Prompt for password when in Sleep Mode", "Promp for password when formatting" and "Prompt for password when upgrading." Use "Space-1" and "Space-4" to toggle these buttons between "Yes" and "no". When you have chosen your options, press "Enter" on the "Confirm" button to save your settings. If you want to cancel the configuration, press "Enter" on the "Cancel" button.

3.8.3 Reset Password to factory defaults.
Use this option to reset the password configuration and return your unit to its factory state of no password protection.
When you press "Enter" to open this option, you are prompted, "Do you want to initialize the password settings?". Use "Space-1" and "Space-4" to choose between "yes" and "No". If you choose "yes", you are prompted for your current password. Type it, and press "Enter". The unit announces, "Password settings have been initialized" and you are placed on the "Set Password" option. 

3.9 Global Options
The "Global Options" on the U2 is a large dialog box for controlling many preferences/settings. You can access "Global Options" from the main menu, by navigating to the "Settings" menu and pressing "Enter". In the "Settings menu, navigate to "Global Options" by pressing "Space-4" or "Space-1" and press "Enter".  You can also open "Global Options" from anywhere on the notetaker by pressing "Space-O". 
You can navigate among the items in "Global Options" using "Space-1" and "Space-4" or using the scroll keys.  You can also use shortcut keys to quickly move to specific items in the "Global Options" dialog. You can toggle an option on or off or cycle through the available values of a setting with the "spacebar" or "Backspace" keys.
Many of the Global Options also have global hotkeys allowing you to adjust these settings from anywhere on the unit. You can view the shortcut and hotkey for an option by placing your cursor on it and pressing "Space-3-6".
To save the changes you've made to the "Global Options" settings, press "Enter" or tab to the "Confirm" button and press "Enter". When you press "Enter" to save the settings, the U2 says, "Saved options," and you are returned to the place on the notetaker from which you entered the "Global Options". To cancel without saving changes, press the "F 4" key, "Space-E" or "Space-Z". The U2 announces, "Canceled saving options". 

3.9.1 Global Options Overview
The "Global Options" dialog contains five groups, making it easy to jump to a particular section in the very long list of settings present in the dialog. the groups are: Braille settings, Voice settings, Display settings, Print settings an  General settings 
You can navigate among the five groups by pressing "page down ("Space-3-4-5" or "F3-F 4")" or "page up ("Space-1-2-6" or "F1-F2")". When you navigate to a particular group, you are placed at the location in "Global Options" where that group of options begins. Though the "Global Options" dialog is divided into groups for ease of navigation, it is actually one long continuous list of settings which you can also move through using normal list navigation. 
* Note: In addition to navigating by group, you may also use shortcut keys to jump to specific settings in the "Global Options" dialog. However, it should also be noted that often, the same shortcut key is used for multiple options. Thus, as is the case when using first letter navigation, pressing a shortcut key moves the focus to the first setting that matches the shortcut key, pressing the key again moves to the next setting that matches that shortcut key. If there are no more settings matching the shortcut key, the U2 wraps around to the first match.

3.9.2 Global Options in Detail

3.9.2.1 Braille display
The first item in "Global Options" is "Braille display". When your cursor is placed on this option, you can toggle the Braille display on and off by pressing "Space". The default setting is "On". Use "B" to quickly jump to the Braille display option. You can also toggle the Braille display on/off from anywhere on the U2 by pressing "Backspace-F3". 

3.9.2.2 Braille Cursor
Use this setting to define how you want the Braille cursor to appear on the Braille display. By default the cursor is set to "Always up". Press "Space" to change the cursor to "Blinking," and again to turn the cursor "Off". 
Use C to jump quickly to this option. Use "f 4-UP scroll" to change the appearance of the Braille cursor from anywhere on the unit.
Note that the Braille cursor can appear in 3 different forms:
Blinking "dots 7-8" is displayed when you are using "overwrite mode" in the word processor. Blinking "dots 1-2-3-4-5-6-7-8" appears when you are selecting text to denote the end of the selection. In all other situations, the cursor is displayed as "dots 7-8".

3.9.2.3 Eight Dot Mode
You can choose to use 6-dot-Braille or 8-dot-Braille mode when entering ASCII text. The shortcut key is "E". By default 8-dot-Braille is set to off. WHEN your cursor is placed on this option, you can turn on 8-dot-Braille mode by pressing "Space". You can toggle this option on/off by pressing "F1-DOWN scroll" from anywhere.

3.9.2.4 View/input Braille Grade 
This option lets you choose what grade of Braille you want to use when viewing/entering text. The shortcut key is "G". The available settings are Uncontracted Braille, Contracted Braille, and Computer Braille. You can cycle among the settings by pressing "Space". You can press "Space-G" to cycle through the Braille grades from any location on the U2.  

3.9.2.5 Braille Code
The Braille code setting defines the rules by which Braille is translated to text and vice versa. The U2 offers 3 English Braille codes as well as entry of Spanish, French, Italian, and German Braille. Thus the Braille code can be set to use "US", "UK", "UEBC", (Unified English Braille Code) or "Spanish", "French", "German", or "Italian". 
Choosing one of the other 4 languages allows you to input Braille according to that language's Braille rules, and read documents created in that language using the associated Braille translation. The Braille language also affects, lists, combo boxes, and edit boxes. Buttons and static boxes are not affected by the change in Braille language.
The short cut key used to jump to the Braille code option is C. The default setting is "US". USE "Space" to cycle through the available codes. You can cycle through all the available Braille codes from anywhere on the unit using "Backspace-Enter-B". 
* Note: If you change the Braille Code option while you are editing Braille in the Word Processor, the meaning of the Braille in your current document will be changed to reflect the current Braille Code setting. To avoid this problem, the Braille Code option should be changed before launching the Word Processor.

3.9.2.6 Line Breaks
When you read a document, if Line breaks are turned off, you can move to the previous/next word one by one and the display scrolls continuously without regard to the line placement. 
For example, when creating a new document from the "File Manager", you are prompted, "New document folder name", first, you see "New document" on the Braille display. When you press "Space-6" or "Space-5", the display shows "document folder". When you press "Space-6" or "Space-5" once again, it changes to "folder name".
When Line breaks are on,the display moves automatically to the next Braille display length of text. 
Use "Space" to toggle line breaks on or off. Use "a (Dot-1)" to quickly jump to "line breaks" from anywhere in "Global Options".

3.9.2.7 Message Display Time
This option defines how the U2 deals with system messages. You can set the unit to ignore system messages, to stand by until you press a key, or, if the Braille display is on, you can define how long the message remains on the display before automatically disappearing. Use M to quickly jump to this item. 
The available settings are "Stand by," "Ignore", and display times of 1 to 10 seconds. The default setting is "3 seconds". Use "Space" to increase the message display time by one second and "Backspace" to decrease the message display time by one second.  If you read the message before the display time has elapsed, you can clear the message by pressing any key. 
Set the unit to standby mode by pressing "Space" until you reach "Stand by". In this mode, the message remains indefinitely until you press a key.  If you choose "Ignore," messages are ignored and do not appear on the display. 

3.9.2.8 Language
The U2 can output speech in English, Mexican Spanish, French, German, Italian and UK English. You can change the Text-to-Speech (TTS) engine using the "Language" setting in the "Global Options" dialog. 
When you change the language of the text to speech engine using this setting, menu items, prompts, and static boxes are not affected and remain spoken in English. However, list items, combo boxes, and all edit boxes and multi-edit boxes, such as documents or e-mail messages, are spoken and text is entered using the language chosen with the "Language" setting. 
When text is entered using a given language, the language attribute is attached to that text, and whenever it is encountered on the unit, it is spoken using the TTS of the language in which it was created. You can change the language associated with a certain block of text using the "Edit Language Attribute" function described in section 5.2.15 of this manual.
The shortcut for jumping quickly to the "Language" setting is L. Press "Space" to cycle through the TTS languages.
* Note: you can change the TTS language from anywhere on the unit by pressing "Backspace-Enter-V". 

3.9.2.9 Voice
This option allows you to toggle the U2 voice on and off. The shortcut key is "V". By default the voice is set to on. You can change the status of the voice by pressing '"Space". You can toggle the voice on and off from anywhere on the U2 by pressing "Backspace-F2". 
You can also hold down "dots 1-2" while turning on the U2, to turn it on without speech. YOU can hold down "dots-1-2" when resetting the U2, to reset it without speech.

3.9.2.10 Punctuation Level
Use this setting to choose how you want the U2 to read punctuation marks. The shortcut key is "P". The available options are "All," "Off", "Punctuation," and "Symbol". The default setting is "Off", thus, by default, the U2 speaks no punctuation marks or symbols. Use "Space" to cycle through the four settings. If you select "All", the U2 speaks all punctuation marks and symbols. When the option is set to "Punctuation", the U2 speaks punctuation marks; when the "Symbol" option is chosen it speaks all symbols and no punctuation marks. 

3.9.2.11 Keyboard Echo
With this option, you can define what the U2 speaks as you type. The shortcut key is K. The setting values are "On with characters and words," "On with characters," "On with words," and "Off". The default is "On with characters and words," thus each keystroke is announced and each word is spoken when "Space" is pressed. If you select "On with characters," each keystroke is announced as you type it. If you select the "On with words" option, each word is spoken after "Space" is pressed.  

3.9.2.12 Capitalization alert
Use this option to choose how the U2 alerts you that a character is capitalized, either when typing or when navigating a document or edit box by character using "Space-3" or "Space-6". The shortcut key is U. The setting values are "Off", "Say cap," and "Pitch". The default value is "Pitch". If you select the default, when you encounter a capital letter, the pitch of the voice is raised to indicate it. If you select "Off", the voice remains the same regardless of upper or lower case. And if you select the "say cap," option, "cap" is spoken before the letter to indicate capitalization. 

3.9.2.13 Numbers
This option defines how you want the U2 to speak numbers. The shortcut key is N. The default value is "On". If "numbers" is set to "On", "2007" is read as "two thousand seven". If "numbers" is set to "Off", numbers are spoken as digits, and "2007" is read as "two zero zero seven". You

3.9.2.14 Abbreviations
You can turn the translation of acronyms on/off on U2. Use "A" to jump quickly to the "Abbreviations" option. If "Abbreviations" is set to "On", when the U2 encounters "Ala" it speaks "Alabama". But if "Abbreviations" is set to 'Off', it speaks "Ala". 

3.9.2.15 Voice Volume
Use this option to set the volume level of the U2's voice. The shortcut key is "L". The volume level can be set using values 1 to 21, with 1 being the lowest volume level and 21 being the highest. Use "Space" to increase the volume by1 increment, and "Backspace" to decrease it. 
FROM anywhere on the U2, you can increase the volume with "Backspace-F 4" and decrease it with "Backspace-F1".

3.9.2.16 Voice Rate
This option controls the rate of the U2's speech. The shortcut key is "R". You can set the rate using values 1 to 12, with 1 being the slowest, and 12 being the fastest.  
From anywhere on the U2, you can increase the speech rate using "Space-F 4" and you can decrease it with "Space-F1". 

3.9.2.17 Voice Pitch
Use this option to control the pitch of the U2's voice. The shortcut key is "T". The available values are 1 to 10, with 1 being the lowest pitch and 10 being the highest.    
From anywhere on U2, you can increase the pitch by pressing "Enter-F 4," and decrease it by pressing "Enter-F1".

3.9.2.18 Sub Voice Rate
The Sub Voice rate option controls the rate of the voice used to output speech in languages other than English. The values range from levels 1 to 12, with the default set to 8. Use "Space" to increase the Sub Voice rate and "Backspace" to decrease it. The shortcut key is "Rather". 
Adjust the Sub Voice rate from anywhere on the U2 using "Space-Enter-F1" to decrease it, and "Space-Enter-From 4" to increase it. 

3.9.2.19 Main Volume
Use the Main Volume option to control the master volume of the unit. Adjusting the Main volume changes the level of both system audio as well as TTS. The available values are 1 to 21.  The shortcut is "V". You can also adjust the main volume from anywhere on the unit by pressing "Backspace-Space-F1" to decrease it, and "Backspace-Space-From 4" to increase it.

3.9.2.20 Scroll Voice
Use this setting to choose whether you want the U2 to speak while using the scroll buttons as you read. The shortcut key is "S" with the default set to "Off". This means the U2 does not speak when you use the scroll keys to move through a document. Set this option to "On" if you would like to hear the U2 speak text as you scroll through it.  

3.9.2.21 Flip LCD display
The U2 gives you the option of viewing the text on the LCD screen in normal or reverse orientation. By default, "flip LCD" is set to "Off", meaning the text is shown in normal orientation. If the option is set to "On", the text is in reverse orientation so that someone across the table can view the display in the correct orientation from his/her position. (Note: this option only appears if the LCD is connected.) 
This is a useful tool for teachers or parents wanting to view a student's work, or for communicating with deaf-blind users.   

3.9.2.22 LCD Font Size
Use this setting to change the font size of the text on your LCD. The shortcut key is "F". The default is set to 19. The font size can be set using values 12 to 20. Use "Space" to increase the font 1 size, and "Backspace" to decrease it. If you have the font size set to 20, and you increase the font by one size, the font wraps around to 12. If your font size is 12, and you decrease the font by one size, the font wraps around to 20. (Only appears if LCD is connected.)

3.9.2.23 Printer Port
Use this option to define which port is used to send information to your printer when printing a document. The shortcut key is P. The default is set to "USB". You can also choose to print via a parallel or Bluetooth printer. 
* Note: if you want to use a parallel port printer, you must use a USB to parallel adapter and connect the printer to the USB port on the U2.  

3.9.2.24 Print Paper Size
This option allows you to select the size of the paper that an ink printer is using so the document is scaled correctly when printing. To jump quickly to this option, use S. The available sizes are "Letter" (8.5 inches by11 inches) and "Legal" (8.5 inches by14 inches.)

3.9.2.25 Audio alerts
Use this setting to choose whether the U2 alerts you to various events using audio signals, vibration signals, both, or no signal. The shortcut key is "A". Audio or vibration alerts may be useful if the speech on the U2 is turned off. By default, "Audio alerts" are turned "On". When "Audio alerts" are set to "beep", you hear a beeping sound when you type keystrokes that are not acceptable in your current context on the U2. If alerts are set to "vibrate motor" the unit emits a vibration as a warning. If the setting is set to "both", you receive both an audio and vibrating alert. If you don't want to hear or feel a warning or alert, press "Space" until you reach the "Off" setting.

3.9.2.26 Play Power On/Off Sound
Use this option to choose whether you hear a sound when you turn on/off the U2. The shortcut key is S. The default is set to "On". 
If you want the U2 to power on/off silently, press "Space" to turn "Off" "Play power on/off sound".

3.9.2.27 Left Scroll Buttons
Use this setting to define the operation of the left scroll buttons. The available options are "Scroll display", "Move by line", "Move by character", "Move by paragraph" and "Move by sentence".   
If you set the value to "Scroll display," the left-scroll buttons scroll by previous/next Braille display length. Pressing the left-up scroll button, scrolls to the previous Braille display length, and pressing left-down scroll button, scrolls to the next Braille display length.
If you set the value to "Move by line", the left-scroll buttons scroll to the previous/next line, similar to pressing "Space-1" or "Space-4" on the Perkins keyboard. 
If you set the value to "Move by character," the left-scroll buttons move to the previous/next character on the Braille display, similar to pressing "Space-3" or "Space-6".
If you set the value to "Move by paragraph," the left-scroll buttons can be used to move to the previous/next paragraph, similar to pressing "Space-2-3" or "Space-5-6". 
If you set the value to "Move by sentence," the left-scroll buttons scroll to the previous/next sentence, similar to pressing "Space-2-3-5" or "Space-2-5-6" on the Perkins keyboard.

3.9.2.28 Right Scroll Buttons
This option defines the operation of the scroll buttons on the right side of the Braille display. The values are exactly the same as those just described in 3.9.2.28 for defining the operation of the left-scroll buttons. .  

3.9.2.29 Skip Empty Lines
You can choose to have the U2 alert you to a blank line by announcing "Blank" as you encounter empty lines while scrolling through a document or you can choose to have the unit skip empty lines. The shortcut key is "E" and the default is set to "Off".    

3.9.2.30 Control Information
Use this setting to determine where information is announced regarding the type of control on which you are currently located, a list item, menu, combo box, etc. The short cut key is "I" and the default is set to "After". To toggle "Control information" between before, after and off, press "space.
If you select "Before," control information, such as "list item", or "combo box" is spoken before a menu/list item or form control. If you select "After," control information is announced after the item or control. If you have control information set to "Off", control information is not displayed or spoken.
* Note: if Control Information is set to anything other than "Off", it always appears in Braille before the control. 
Note that if you are using the Web browser the control symbols are displayed even if the "Control information" option is set to "Off".  

3.9.2.31 Hide passwords
When you enter a password in a computer edit box, The U2 can either display an asterisk, (dots 1-6) or the actual password as you type it. 
The short cut key is P and the default is set to "On". This means passwords are hidden, and thus will be shown using asterisks. To show passwords as you type them, use "Space" to toggle this setting to "Off". 

3.9.2.32 Hot Key Information
Use this option to define how hot key information is announced. The short cut key is "H" and the default is set to "Letters". The available settings are "Letters," "Dot patterns," and "Off". 
If you select "Letters," the "Open" option in the File Menu of the Word Processor is announced, "Open (o) Enter-o". If you select "Dot patterns", it is announced, "Open (o) enter dots 1 3 5". And if you select "Off", the hot key information is not announced. 

3.9.2.33 Announce shortcut keys
The "Announce shortcut keys" option lets you choose whether the U2 speaks the menu shortcut key for a function. The shortcut key for this option is "S" and the default is set to "On".  If you do not wish to hear the shortcut keys announced, toggle "Announce shortcut keys" off by pressing "Space".

3.9.2.34 Power Saving Mode
Use this option to set the U2 to save power by automatically shutting down after a certain period of time. The shortcut key is "P". The default setting is set to "On". USE "Space" to cycle through "On", "Off", and "Message". If you never want your U2 to shut down automatically, set the option to "Off". If you set the option to "Message," The U2 gives you a warning message that says "power on" to remind you the unit is still powered on after 10, 20, or 30 minutes of inactivity (depending on the setting that you choose for power saving kick in). 
* Note: this option is available only when the AC adaptor is not connected to the unit. In other words, even if this option is set to "On", if the AC adaptor is connected to the unit, the unit does not enter Power Save Mode, even when the "Power saving kick in" time has elapsed.

3.9.2.35 Power Saving Kick In
Use this option to set the time of inactivity before entering Power Save Mode. The shortcut key is K with the default set to "After 10 minutes". This means the U2 enters power saving mode when you have not used the U2 for 10 minutes. Use "Space" to cycle among 10 minutes, 20 minutes, and 30 minutes.

3.9.2.36 Check Today's Schedule
You can use the "Schedule Manager" to keep track of your appointments. You can set the U2 to check today's schedule for appointments each time you turn it on. The short cut key for this option is S. Press "Space" to toggle this option on/off.

3.9.2.37 One-Handed Mode
This option allows users with only the use of one hand to use the U2 in a specific mode adapted for that purpose. The shortcut key is H. The default setting is "Off".  For detailed information about one-handed mode, refer to "2.14 One-Handed Mode".
* Note: If this option is set to "On" when you connect a USB keyboard, it is automatically turned off when the keyboard is connected. The option returns to its previous state when the USB keyboard is disconnected from the unit. 

3.9.2.38 Enable spell-check
This option allows you to choose whether or not spellcheck is enabled on the unit. You may wish to disable it, specifically in educational situations where a student needs to b tested on spelling, etc.
The shortcut is C. By default, Enable Spellcheck is turned on. 
* Note: If "Enable Spellcheck" is turned off Automatic Spellcheck cannot be used.

3.9.2.39 Automatic spell-check
Use this option to set whether the U2 automatically checks spelling as you type in "multi line edit boxes" in programs such as the Schedule Manager, Address Manager, E-mail messages, the Word Processor, etc. The short cut key for this option is C. 
By default this option is set to "Off", thus spelling is not automatically checked as you type.  If the option is "On", and you enter a misspelled word, U2 emits a beep sound to indicate a misspelling. This beep sounds even if audio alerts are turned off.

3.9.2.40 Default Document Type
This option is used to set the default document type for new documents you create using the word processor on the U2. The shortcut key is Q. By default, "Text document" is selected as the default file type. 
You can choose "Sense document", "Braille document," or "Text document" as your default document type.  
* Note: When you connect a USB QWERTY keyboard to the U2, this option is automatically set to "Text document". When the USB keyboard is disconnected, the default document type is returned to whatever it was set to before the USB keyboard was connected.

3.9.2.41 Default Browser
This option allows you to set whether to use the original Sense Web Browser or the newer Quick Browser as your default browser for opening web pages from programs such as E-mail, RSS, Google Search, and Twitter. 
The shortcut key for this option is B. By default, this option is set to the "Quick Browser". 

3.9.2.42 Automatically synchronize with time server
If you have this option turned on, the date and time is synchronize with an internet time server automatically each time the U2 is connected to internet. Using this feature, you can ensure the accuracy of the time on the U2 by synchronizing with an atomic clock. 
The shortcut key is T. The default setting is "ON".   

3.9.2.43 Time Announcement
The "Time Announcement" option allows you to have the time announced every 30 minutes or every hour if you wish. 
By default, this option is set to 'Off". The shortcut is T.

3.9.2.44 Progress indicator
The progress indicator setting defines how the progress of opening a document, copying files or opening a webpage is indicated. The shortcut key is P. You can choose among "Silent," (no progress indication) "Beep," (continuous beeps while the task is performed) and "Message" (progress is shown as a percentage).  By default, progress indication is set to "Message". People 

3.9.2.45 Bluetooth
Use this option to turn Bluetooth on or off. The shortcut key for this option is B.  By default, it is set to "Off". You can toggle Bluetooth on and off from anywhere on U2 by pressing "Backspace-3-4-5-6". 
* Note: It is recommended that you turn Bluetooth off when it is not in use to save battery power.

3.9.2.46 Wireless LAN
Use this setting to turn Wireless LAN on or off. The shortcut key is "W". By default, wireless is set to "Off". You can toggle it on and off from anywhere on U2 by pressing "Backspace-1-4-5-6" 
* Note: you must turn Wireless LAN on before connecting to a wireless network or to the internet via a wireless router. It is recommended that you turn wireless off when not in use to save battery power.

3.9.2.47 Mass-storage device mode
Mass Storage Device Mode enables the drives on your U2 to be viewed as removable storage devices on a PC when connected via USB. The shortcut key for this option is "D" with the default set to "On".  
If Mass Storage Device Mode is turned off, the U2 can be connected to the PC as a Windows Mobile device and accessed using Microsoft ActiveSync or Windows Mobile Device Center for synchronization of calendar and contacts with Outlook.

When you have finished modifying settings in the "Global Options" dialog, press "Enter" to save the settings. You can also "Tab" to the "Confirm" button, and press "Enter". If you do not want to save the settings, "tab" to the "Cancel" button, and press "Enter". You can also cancel saving the settings by pressing "Space-Z" Or "Space-E".
