
TABLE OF CONTENTS

13. Bluetooth Manager
13.1 Bluetooth Device List
13.2 Bluetooth Service List
13.2.1 Connecting  a Service
13.2.2 LAN Service
13.2.3 FTP Service
13.2.4 ActiveSync Service
13.2.5 Serial Port
13.2.6 Bluetooth keyboard service
13.2.7 Bluetooth Printer service
13.2.8 Using Multiple Services
13.3 Hot keys in Bluetooth Manager

13. Bluetooth Manager

The Braille Sense U2 is Bluetooth capable, or rather, you can connect the Braille Sense U2 to various devices such as keyboards, printers, audio devices, and other computers without the need for cables. . Bluetooth is the latest in wireless technology and enables wireless connectivity via a Personal Area Network (PAN). Unlike a traditional Wireless Local Area Network (WLAN), these networks are limited to approximately 30 feet or less. Bluetooth enables users to exchange various types of information over this wireless connection. 
To use Bluetooth with the Braille Sense U2, you must first turn the Bluetooth option "On" in the "Global Options" dialog. You can also toggle Bluetooth on/off from anywhere on the unit using "Backspace-dots-3-4-5-6".  
You can use Bluetooth to transfer files from the Braille Sense U2 to a computer, use your computer's Internet connection, or use the Braille Sense U2 as a wireless Braille display for a computer or smart phone. Note: to use the Braille Sense U2 as a wireless Braille display, you must be running a screen readers such as Window-Eyes, Supernova, or VoiceOver. Please note that Bluetooth is an evolving standard, and the functionality may vary , depending on the operating system that you are using.
The Braille Sense U2 uses the built-in Bluetooth Manager program to manage Bluetooth functionality. You can access the Bluetooth Manager in several ways. To access Bluetooth Manager from the program menu, press "Space-1" or "Space-4" to navigate to Bluetooth Manager, or press "Space" until you reach Bluetooth Manager. When your cursor  is placed on Bluetooth Manager, press "Enter" to activate it. You can also press "l (dots 1-2-3)" to jump to and open the Bluetooth Manager from the "program" menu. 

13.1 Bluetooth Device List

When the Bluetooth Manager is activated, it begins scanning for other Bluetooth devices that are in range, and the services available from the other Bluetooth devices. For example, if you have a computer with Bluetooth enabled nearby, the Braille Sense U2 attempts to find it. It may take 30 to 40 seconds to discover all of the Bluetooth devices in range. The Braille Sense U2 announces and displays, "Scanning for devices. Please wait...". Progress beeps are heard during the scanning process, and full cells are filled in on the Braille display to indicate scanning progress. 
When a Bluetooth device is detected, the Braille Sense U2 announces "found (Bluetooth device name)". Note: while the Braille Sense U2 is scanning for Bluetooth devices, it cannot respond to key presses. In addition, you may not cancel the scan once it has begun, but must wait for its completion before the Braille Sense U2 returns to normal operation.  
If Bluetooth is turned "Off", or if the Braille Sense U2 does not recognize the Bluetooth radio, the Braille Sense U2 announces, "Bluetooth not activated", and  exits the Bluetooth Manager.

When the scanning process completes, you are placed in the Bluetooth Device List. If the Braille Sense U2 has found other Bluetooth devices in range, they are displayed as "device name (untrusted (or trusted)) xx/yy" where xx is the number at which the device appears in the list, and yy is the total number of devices. "Trusted" indicates that the service has been authenticated, "untrusted" indicates the service has not been authenticated.
If there are no other Bluetooth devices in range, the Braille Sense U2 announces, "no items". You can press "Space-1" or "Space-4" to move through the list. To select a device from the list, press "Enter" on the device name.
If the Bluetooth device is trusted, settings for connecting the device are automatically saved in the Braille Sense U2. If you want to delete this information, press "Space-d (dots 1-4-5)" on the Bluetooth device name in the Bluetooth Device List. The Braille Sense U2 announces, "Device settings removed". Removal of the settings applies only to the current device.
From the Bluetooth Device List, you can access the menu by pressing "Space-m (dots 1-3-4)" or by pressing "F2". The "Bluetooth Device List menu" contains "Rescan For Devices", "Device Name", "Delete Pair Information", and "Exit". You can navigate among the menu items using "Space-1" or "Space-4".
The first menu item is "Rescan For Device". This option initiates a new scan for other Bluetooth devices. To activate this item, press "Space-m (dots 1-3-4)" or "F2" and press "Enter" on "Rescan For Device". You can also access this option by pressing "r (dots 1-2-3-5)" from within the Bluetooth Device List menu, or you can activate it directly by pressing "Enter-r (dots 1-2-3-5)".
You can access the next item in the menu by pressing "Space-m (dots 1-3-4)" and "Space-1" or "Space-4" until you reach "Device Name", and press "Enter". You can also press "n (dots 1-3-4-5)" from within the menu to activate the "Device Name" option. You can access it directly by pressing "Enter-n (dots 1-3-4-5)". 
This item allows you to specify the device name given to the Braille Sense U2. The default name for the Bluetooth device name is "BrailleSenseU2".  When you activate this option, you are placed in a computer edit box that contains your current device name. To modify the name, type the new name and press "Enter". After entering the new name, you should close all programs and reset the Braille Sense U2 by pressing the "Reset" button on the rear panel of the unit. To cancel your changes, press "Space-e (dots 1-5)" or "F 4". You are returned to the Bluetooth Device List.
The next menu item is "Delete Pair Information". This item allows you to remove the connection settings for the current device. To activate this item, press "Space-m (dots 1-3-4)" or "F2" and press "Enter" on "Delete Pair Information". You can also access this option by pressing "d (dots 1-4-5)" from within the menu, or you can activate it directly by pressing "Space-d (dots 1-4-5)".
The final item in the Bluetooth Device List menu is "Exit". This option exits the Bluetooth Manager program. To activate this item, press "Space-m (dots 1-3-4)" and press "Space-1" or "Space-4" to navigate to "Exit" and press "Enter". You can also access "Exit" by pressing "z (dots 1-3-5-6)" from within the menu. Exit the program any time by pressing "Space-z (dots 1-3-5-6)".

13.2 Bluetooth Service List

When you locate a Bluetooth device to which you'd like to connect, press "Space-1" or "Space-4" to navigate to the device in the Bluetooth Device List, and press "Enter" on the device name. The unit announces, "Scanning for services. Please wait...". Please note The Braille Sense U2 does not respond to key presses during the scanning process. 
The Braille Sense U2 supports the following Bluetooth services: LAN, FTP, ActiveSync, Serial port, USB port, headset, and Bluetooth DUN. To access any of these functions, be sure that the remote Bluetooth device is in Discoverable mode, and that the service you wish to access is enabled on that device. It is possible to have certain services enabled on your remote Bluetooth device, while disabling others. For example, you could have LAN and FTP enabled, while having ActiveSync and Serial Port disabled. The Braille Sense U2 only sees and displays services which are enabled on your remote device, even if others are available. 
When the Braille Sense U2 has found all of the available services, the services are displayed in a list in the following format: "service name xx/yy" where xx is the number at which the service appears in the list, and yy is the total number of available services. You can move through the available services by pressing "Space-1" or "Space-4". Press "Backspace" to return to the Bluetooth Device List.
From the Bluetooth Service List, you can access the menu by pressing "Space-m (dots 1-3-4)" or by pressing "F2". The "Bluetooth Service List menu" contains "Device Name", "Open FTP", "Disconnect" and "Exit". You can navigate the menu items using "Space-1" or "Space-4".
The "Device Name" and "Exit" options in the "Bluetooth Service List" menu are the same as those in the "Bluetooth Device List" menu. 
The "Open FTP" menu item allows you to quickly open a direct FTP connection with a remote Bluetooth device without accessing the Device and Service lists. However, you must have connected the FTP service previously for the Braille Sense U2 to allow you to transfer files. If you have not connected the FTP service, and you activate this function, the unit announces, "FTP service disconnected". 
You can access "Open FTP" by pressing "Space-m (dots 1-3-4)" then use "Space-1" or "Space-4" to navigate to "Open FTP" and press "Enter". The Braille Sense U2 says, "Connecting service". You can also activate it by pressing "t (dots 2-3-4-5)" from within the menu, or by pressing "Enter-t (dots 2-3-4-5)" directly from the Bluetooth Service List. Connecting various Bluetooth services is covered in more detail later in this chapter.
The "Disconnect" menu item allows you to disconnect services with other Bluetooth devices. You can access this item by pressing "Space-m (dots 1-3-4)" and "Space-1" or "Space-4" to navigate to "disconnect". Press "Enter" to activate it. You can also activate this item from within the menu by pressing "d (dots 1-4-5)". Or you can activate it directly from the Bluetooth Service List by pressing "Enter-d (dots 1-4-5)".
To disconnect a service, press "Space-1" or "Space-4" to navigate to the service in the Bluetooth Service List and execute the "Disconnect" command.
If there are no services connected and you activate this function, the unit says, "There is no service connected".

13.2.1 Connecting  a Service

To authenticate a service and connect to it, press "Enter" on the service. The Braille Sense U2 announces, "Connecting service". You are then prompted for a "PIN code:" You must use ASCII characters when you type the pin code. This edit box only appears when you have not previously connected to a service, and a pin code is required by the device. You can exit the edit box or delete text you have typed by pressing "Space-z (dots 1-3-5-6)", and you are returned to the Bluetooth Service List.
When you finish typing the pin code, press "Enter". The unit announces, "Please wait for authentication". If the remote device is setup correctly, and has not been set up to allow this device to always connect, the remote device also asks for a pin code. Please be sure to enter the same pin code on both devices. If the remote Bluetooth device pin code matches the pin code on the Braille Sense U2, the service should authenticate. If connection is successful, the unit announces, "PIN code authentication accepted". 
You are then prompted, "Please wait. Access permission". If the remote Bluetooth device does not give access permission, the unit says, "Connection failed", and you are returned to the Bluetooth Services List. If the remote Bluetooth device gives you access permission, the Braille Sense U2 says "Connection succeeded". If the connection succeeds, "Connected" is displayed after the service in the Bluetooth Service List. Some services may be connected without inputting a pin code depending on the Remote Bluetooth device settings.
When you are connected to a service, you can press "Enter-d (dots 1-4-5)" to disconnect the service. The Braille Sense U2 says, "Service disconnected", and you are returned to the Bluetooth Service List. 
If you connect to the FTP service, a list of files and folders on the remote Bluetooth device is displayed. The rest of this chapter discusses each service in detail.

13.2.2 LAN Service

You can use the LAN service to access the Internet via your computer's Internet connection. If you connect this service, you can use the Web browser and email program, as if you were connected to the Internet via Ethernet or wireless LAN. Before you can connect to the LAN service on a remote Bluetooth device, the device must be configured for Internet Connection Sharing (ICS). If ICS is not properly setup, you cannot connect to the Internet using the LAN service. For information on how to setup ICS for your remote Bluetooth device, please refer to the documentation that came with your Bluetooth adapter. Setting up ICS requires knowledge of network architecture, so it may be a good idea to contact a local network technician or your network administrator for help with setting up ICS.

13.2.3 FTP Service

This service works similarly to using FTP on the Internet. It allows you to transfer folders and files to and from the remote Bluetooth device. When referring to the FTP service, we will refer to the file/folder list on the remote Bluetooth device as the "remote folder list" and the file/folder list on the Braille Sense U2 as the "local folder list".
After you have successfully connected to the FTP service, the Bluetooth Manager places you in the remote folder list. The remote folder list displayed is determined by the remote Bluetooth device. Typically, this folder is called the Bluetooth Exchange Folder, but you should check your remote Bluetooth device documentation for definitive information. 
You can interact with the remote folder list in much the same way as you interact with files and folders in the File Manager. With the FTP service, you can perform the following functions:
1. Copy
2. Paste
3. Send To
4. Retrieve File
5. New Folder
6. Delete File/Folder
7. Open Local Folder. If you press "Enter" on this option, you are taken to the local folder list. If you are in the local folder list, this menu option changes to "Move to remote folder".
8. Select All
9. Information
In the next few sections, we will discuss the various FTP functions. Please note that while sending data to and from the remote Bluetooth device, the remote Bluetooth device may still need to give access permission to the Braille Sense U2. Please consult the documentation for the remote Bluetooth device for details.

13.2.3.1 Copy and Paste

These functions allow you to copy and paste files between the local folder and the remote folder.
Use the following steps to copy files from a local folder to the remote folder:
1) From the remote folder list, press "Space-m (dots 1-3-4)" or "F2" to open the FTP menu. Press "Space-1" or "Space-4" to navigate to "Open Local Folder", and press "Enter". You can also press "o (dots 1-3-5)" while in the menu, or you can press "Enter-o (dots 1-3-5)" to open the local folder directly from the remote folder list. After activating this function, the unit says, "Opening Local Folder", and you are placed  in the Disk list that appears in File Manager. You are placed on "flashdisk" by default, but if you have an SD card or USB memory stick inserted, you can navigate to them by pressing "Space-1" or "Space-4".
2) As when navigating in the File Manager, you can access a disk by pressing "Enter" on it. Use the same navigation keys as in the File Manager to navigate the local folder. Note that you cannot select folders. You can only select files. If you try to select a folder, the Braille Sense U2 says, "Deactivated".
3) Once you have selected files by pressing "Space", you can copy them by pressing "Space-m (dots 1-3-4)" or "F2", and navigate to "Copy" by pressing "Space-1" or "Space-4", and press "Enter". Or, you can press "Enter-c (dots 1-4)". 
4) After you have activated the copy command, Braille Sense U2 announces, "Copying" and "Open Remote Folder". You are then returned to the remote folder list.
5) In the remote folder list, navigate to the folder where you want to paste the file. Press "Enter-v (dots 1-2-3-6)". Or, you can press "Space-m (dots 1-3-4)", and use "Space-1" or "Space-4" to navigate to the "Paste" function, and press "Enter". If the file is larger than 300 KB, progress messages are spoken each time an additional 10% is completed. If the file is less than 300 KB, only progress beeps are heard. 
6) When the file is pasted successfully, the Braille Sense U2 displays the message, "xxx file pasted", where xxx is the name of the file. If the file is not pasted successfully, "xxx file not pasted" is displayed. After the file is pasted successfully, the unit also announces, "Paste completed", and you are returned to the remote folder list.

Use the following steps to copy a file from the remote folder list to the local folder list:
1) Navigate the remote folder, just as you would in the File Manager. For information on how to navigate the File Manager, please refer to chapter 4 in this manual.
2) Select the files that you want to copy by pressing "Space", you can open the FTP menu by pressing "Space-m (dots 1-3-4)", and use "Space-1" or "Space-4" to navigate to "Copy", and press "Enter". You can also activate this function by pressing "Enter-c (dots 1-4)". Note that you can only copy files, you cannot copy folders, to send to the local folder.
3) After you have activated the "Copy" function, the Disk list appears as it does in the File Manager. You are placed on "flashdisk" by default. However, if you have an SD card or USB memory stick inserted, you can navigate to those disks by pressing "Space-1" or "Space-4". 
4) After entering a disk, open the menu by pressing "Space-m (dots 1-3-4)". Then, move to "Paste" with "Space-1" or "Space-4", and press "Enter". You can also activate this function by pressing "Enter-v (dots 1-2-3-6)". If the file is larger than 300 KB, progress messages are spoken each time an additional 10% is completed. If the file is less than 300 KB, only progress beeps are heard. 
5) When the file is pasted successfully, Braille Sense U2 displays the message, "xxx file pasted", where xxx is the name of the file. If the file is not pasted successfully, "xxx file not pasted" is displayed. After the file is pasted successfully, the unit also announces, "Paste completed", and you are returned to the local folder list.

13.2.3.2 Send To

This function allows you to send files from the local folder list to the remote folder list. Note: this option is only available in the local folder list. This is very similar to the copy and paste function with a couple of notable differences. One difference is that you do not have to paste the file to the remote folder. It is done as soon as you activate the "Send To" function. ANOTHER difference is that when you activate this function, the file can only be sent to the root of the remote folder list. To copy a file using the "Send To" function, follow these steps:
1) Press "Space-m (dots 1-3-4)" from the remote folder list to open the menu. Then, press "Space-1" or "Space-4" to move to "Open Local Folder", and press "Enter". You can also activate this function directly from the "remote folder list" by pressing "Enter-o (dots 1-3-5)".
2) After you have activated the "Send To" function, the disk list appears as it does in the File Manager. You are placed on "flashdisk" by default. However, if you have an SD card or USB memory stick inserted, you can navigate to those disks by pressing "Space-1" or "Space-4". Please refer to chapter 4 in this manual for information on file and folder navigation.
3) Select a file by navigating to it and pressing "Space". Note: you can select only files; folders cannot be selected.
4) After you have selected a file, press "Space-m (dots 1-3-4)", and press "Space-1" or "Space-4" to move to "Send To", and press "Enter". Or, you can press "Enter-s (dots 2-3-4)" to activate the "Send To" function directly.
5) As with copying and pasting, progress beeps are heard during the send process. If the file is larger than 300 KB, progress messages are spoken each time an additional 10% is completed. If the file is less than 300 KB, only the progress beeps are heard. When the transfer is complete, the unit announces, "xxx file sent", where xxx is the name of the file. If the file does not transfer, the unit says, "xxx file not sent". When all selected files are transferred, the Braille Sense U2 announces, "Successfully sent", and you are returned to the remote folder list.

13.2.3.3 Retrieve File

The "Retrieve File" function allows you to retrieve a file from the remote folder list, and move it to the local folder. This function is only available from the remote folder list. When using this function, all retrieved files are saved to the "flashdisk/download" folder. Use the following steps to retrieve a file: 
1) Navigate the remote folder list using the same commands as in the File Manager (see chapter 4). 
2) PRESS "Space" to select the file you want to retrieve. Note that you can select only files, not folders.
3) After selecting the file, press "Space-m (dots 1-3-4)" to open the menu, and use "Space-1" or "Space-4" to move to "Retrieve File", and press "Enter". You can also activate this function directly by pressing "Enter-r (dots 1-2-3-5)".
4) As with copying and pasting, progress beeps are heard. If the file is larger than 300 KB, progress messages are also spoken each time an additional 10% is completed. If the file is less than 300 KB, only progress beeps are heard. When the transfer is complete, the unit announces, "xxx file retrieved", where xxx is the name of the file. If the file does not transfer, Braille Sense U2 says, "xxx file not retrieved". When all of the selected files are transferred, the message "Retrieve completed" is spoken, and you are returned to the remote folder list.

13.2.3.4 New Folder

The "New Folder" function allows you to create a new folder in either the local folder list or the remote folder list. Use the following steps to create a new folder: 
1) With the FTP service connected, from either the local or remote folder list, navigate to the folder in which you want to create a new folder. Move between the "remote folder list" and "local folder list" by pressing "Enter-o (dots 1-3-5)". Use normal folder and file navigation commands to move among the items in the folder list. 
2) Press "Space-m (dots 1-3-4)" to open the menu, and use "Space-1" or "Space-4" to navigate to "New Folder", and press "Enter". Or, you can activate the "New Folder" function directly from the folder list by pressing "Enter-f (dots 1-2-4)". 
3) An edit box appears and the unit prompts, "New folder name:". Type the new folder name using ASCII characters, and press "Enter". If the folder is created successfully, the Braille Sense U2 says, "xxx folder created", where xxx is the name of the folder. You are then returned to your previous location: either the remote or local folder list.
4) To cancel the folder creation, press "Space-z (dots 1-3-5-6)", and you are returned to the previous list.

13.2.3.5 Delete File/Folder

This function allows you to delete files or folders from the remote or local folder list. Note that if a folder contains sub-folders, you cannot delete the folder. To delete a file or folder, do the following: 
1) With the FTP service connected, navigate to the local or remote folder list, and select the file(s) or folder(s) you want to delete using "Space". You can move between the "remote folder list" and "local folder list" by pressing "Enter-o (dots 1-3-5)".
2) After selecting the file(s) or folder(s) you want to delete, press "Space-m (dots 1-3-4)", use "Space-1" or "Space-4" to move to "Delete File/Folder", and press "Enter". You can also activate the "Delete" function directly by pressing "Space-d (dots 1-4-5)".
3) If the file(s) or folder(s) are deleted successfully, "Delete completed" is spoken.

13.2.3.6 Information

This function allows you to obtain information about files or folders located in the remote or local folder list. You can obtain file or folder information by following these steps:
1) With the FTP service connected, navigate to the local or remote folder list, and select the file or folder about which you want information. 
2) Press "Space-m (dots 1-3-4)" to open the menu, use "Space-1" or "Space-4" to move to "Information", and press "Enter". Or, you can activate the "Information" function directly from the folder list by pressing "Enter-i (dots 2-4)".
3) The "Information dialog box" appears. The dialog box contains "Type", "Size", "Date", "Attribute (except for folders)", and "Close". You can move among these controls by pressing "tab (Space-4-5)" or "shift-tab (Space-1-2)". If you select multiple files, the "Information" dialog displays the number of selected files and  total size.

13.2.4 ActiveSync Service

This service offers the same functionality as connecting the Braille Sense U2 to a computer via USB and using ActiveSync. If the connection to the ActiveSync service is successful, you will hear the chime indicating ActiveSync is successfully connected. As with all of the Bluetooth services, the remote Bluetooth device may need to authorize the Braille Sense U2. You are then returned to the Bluetooth Service list. As with using ActiveSync via USB, you can copy and paste files from the Braille Sense U2 from the remote Bluetooth device to the Braille Sense U2 and vice versa.

To disconnect the service, press "Enter-d (dots 1-4-5)" from the Bluetooth Manager. The Braille Sense U2 says, "Service disconnected", and you are returned to the Bluetooth Service list. 
You cannot use ActiveSync via USB and Bluetooth at the same time. If the remote Bluetooth device is connected via USB and using ActiveSync, you must terminate the USB ActiveSync connection on the remote Bluetooth device in order to use the ActiveSync service via Bluetooth.

13.2.5 Serial Port

If you connect this service, you should not connect to other Bluetooth services. The Serial Port service allows you to use your Braille Sense U2 as a wireless Braille display via Bluetooth. Note: you must be using Window-Eyes, SuperNova, VoiceOver, or another compatible screen reader to use the Braille Sense U2 as a wireless Braille display. To use the Braille Sense U2 as a wireless Bluetooth display with Window-Eyes or iPhone or iPad, please reference the following sections.  If you are using another screen reader than those addressed below, please contact HIMS by e-mail at support@hims-inc.com. 

13.2.5.1 Setting up the Braille Sense U2 to Work as a Bluetooth Braille Display with Window-Eyes

The following steps will walk you through setting up the Braille Sense U2 to work as a Bluetooth Braille display with the Window-Eyes screen reader from GW Micro. These instructions assume that you already have Bluetooth installed on your computer. The following instructions also assume that you are running Window-Eyes 5.5, or higher, and at least Windows XP, Service Pack 2. Before you begin, make sure that your Braille Sense U2 is turned on. Although it may not be necessary, you should close all running applications on the Braille Sense U2, and be placed in the Program menu for best results. If you have more than one Braille Sense U2, make sure that only the Braille Sense U2 that you want to configure is turned on.

13.2.5.2 Setting up the Computer

1) Navigate to the Bluetooth icon in the System Tray. You may do this in Windows XP by pressing "windows key-b", and use the Right or Left Arrow Keys until you reach the Bluetooth icon. Then, press the "context menu key". Note that if you don't have the Bluetooth icon in the System Tray, you may have to change the settings for the Bluetooth icon to appear. Go to the Windows Control Panel, Bluetooth Devices, Options, and check the check box that says "Show the Bluetooth Icon in the Notification Area".
2) Press the "up or down arrow" keys until you get to "Open Bluetooth settings".
3) Press "Enter".
4) Select the Device tab control. You may need to press Ctrl-Tab in order to select this tab control.
5) Tab to the Add button.
6) Press "Enter".
7) Press "Space" to check the checkbox for "My device is setup and ready to be found".
8) Press enter".
9) The XP machine will find the Braille Sense U2, and it will be called "Windows CE". Remember that the Braille Sense U2 must be turned on in order to be found as mentioned above. If you forgot to turn the Braille Sense U2 on, leave it turned on, exit the Bluetooth settings, and start at step number 1 above.
10) Press the "down arrow" key to focus Windows CE.
11) Tab to the Next button.
12) Press "Enter".
13) Press "down arrow" to focus the radio button, "Let me choose my own passkey". Focus will automatically be put in the edit box, and you may hear a tool tip that says, "We recommend using a passkey that is 8 to 16 digits long". You should type your passkey here. For example, you might type, "1111".
14) Press "Enter". Windows will then begin exchanging the passkeys, and a new dialog will appear on the computer.
15) The Braille Sense U2 will then ask for the passkey by saying, "Computer Edit Box PIN code:" Using the same passkey that was typed in to the computer, type in the same passkey on the Braille Sense U2 and press "Enter" on the Braille Sense U2.
16) The computer should display the message, "Found new hardware" and the final dialog should appear on the computer. Remember that you can press "ctrl-shift-w" to have the entire dialog read using Window-Eyes. The dialog should display that the Bluetooth device was successfully set up. It is very important to note the COM ports for the outgoing COM port and the incoming COM port. For example, the outgoing COM port may be COM 5, and the incoming COM port may be COM 6. Do not be surprised if your COM ports are not set to COM 5 and COM 6. The COM ports used can vary from computer to computer.
17) Press "tab" to get to the Finish button, and press "Enter" to activate it.
18) You will then be taken back to the Bluetooth device settings dialog. Press Ctrl-Tab twice to focus the COM ports tab control.
19) Press "tab" to get to the list of COM ports, and press the Down Arrow to move through the list of COM ports to make sure that they match the COM ports that were mentioned when you completed the Bluetooth device wizard. You should hear your first COM port, then the direction, and the name. After you press "down" Arrow again, you should hear the next COM port, the direction, and name. For example, when you press the "down arrow" key the first time, you might hear, "COM 5 Outgoing Windows CE Blue Tooth Serial". When you press the "down arrow" key a second time, you might hear, "COM 6 Incoming Windows CE".
20) Tab to the OK button, and press Enter.
You have now setup the Braille Sense U2 and the computer. However, you must properly setup Window-Eyes in order to use the Braille Sense U2 as a Bluetooth Braille display.

13.2.5.3 Setting up Window-Eyes

1) Press "ctrl-backslash" to open the Window-Eyes Control Panel.
2) Press "alt-f" to open the File menu.
3) Press the "up arrow", or "down arrow" to move to Select Braille Display, and press "Enter". Or, just press B to open the Select Braille Display dialog without using the Arrow Keys.
4) Press the "down arrow" or the letter b until you hear Braille Sense U2.
5) Press "tab" to get to the COM port list box
6) Select the COM port that was given as the outgoing COM port when you setup the computer to interact with the Braille Sense U2 via Bluetooth.
7) Press "Enter"
Now that you have set up Window-Eyes, you need to return to the Braille Sense U2 to finish the setup. 

13.2.5.4 Setting up the Braille Sense U2

1) Press "F1" to get to the Program menu.
2) Press "Space-1" or "Space-4" to get to the Utilities menu, or just press the letter u".
3) Press "Enter".
4) Press "Space-1" or "Space-4" to get to Terminal for screen reader, and press" enter".
5) Press "Space-1" or "Space-4" to get to Bluetooth Serial Port, and press "Enter".
The Braille Sense U2 should be connected as a Bluetooth Braille display. To exit Terminal Mode, press "Backspace-Space-z". Please note that "F1" on the Braille Sense U2 still takes you to the Program menu as you can continue to multi-task while in Terminal Mode. This enables you to use the applications on the Braille Sense U2 at the same time, and be able to switch back to using the Braille Sense U2 as a Bluetooth Braille display.

13.2.5.5 Using Braille Sense U2 as a Braille display with iPhone, iPad, or iPod

Use the following instructions to connect the Braille Sense U2 as a Bluetooth Braille display with your iPhone, iPad, or iPod. Note: You must be running IOS 4.2 or higher on your i-device in order to use the Braille Sense as a Bluetooth Braille display with VoiceOver. These instructions refer to the iPhone, however, they apply to all compatible i-devices: iPhone 3Gs and higher, iPad, and iPod Touch 3G and later.
On the Braille Sense U2:
1) Turn Bluetooth on using "Backspace-dots-3-4-5-6".
2) From the Program menu, press u to access the "Utilities" menu, then press s to execute Terminal for Screen reader. 
3) Choose "Bluetooth Serial" as your connection type and pres "Enter".
4) Braille Sense U2 displays "connecting" soon followed by "Terminal Mode"

On the I-Phone:
1) Navigate to Settings/General/Accessibility/VoiceOver/Braille.
2) If Bluetooth is not activated on the I-Phone, it will prompt you to do this. WHEN Bluetooth is activated, the I-Phone searches for devices.
3) The Braille Sense U2 should appear in the list of available Braille devices.
4) Double tap the "Braille Sense U2" in the Braille devices list.
5) You are asked for a pin code. Enter any 4 digit code of your choosing.
6) Double tap the "Pair" button.
  
Returning to the Braille Sense U2:
The Braille Sense U2 asks for a pin code. Enter the same pin code you entered into the iPhone and press Enter.
You should hear a chime on the iPhone, and the text displayed on the iPhone should appear on the Braille display of your Braille Sense U2.
For information on operating the iPhone using the Braille Sense as a Braille Terminal, please refer to Apple's accessibility website at www.apple.com/accessibility 
To exit "Terminal for Screen reader" press "Backspace-Space-z (dots 1-3-5-6)".

13.2.6 Bluetooth keyboard service

You can use this service to connect a Bluetooth keyboard to your Braille Sense U2. 
Before you try to use this service, please be sure the Bluetooth keyboard is turned on and in Bluetooth range.
Use the following steps to connect to a Bluetooth keyboard:
1) Navigate to the Bluetooth keyboard  in the Bluetooth Device List and press "Enter". 
2) "Keyboard" should be displayed in the list of available services. 
3) Press "Enter" on the "Keyboard" service.
4) If the keyboard requires a PIN code you are prompted to enter it. Some devices do not require a PIN code, in which case, you are not prompted to enter one. 
5) IF you are prompted, input the  PIN code on the Braille Sense U2 and press "Enter". If the keyboard requires a PIN code, you must also input the PIN code on the Bluetooth Keyboard. (You should be able to locate PIN code information for the Bluetooth keyboard in the documentation that came with it.)

13.2.7 Bluetooth Printer service

You can use this service to print documents from the Braille Sense U2 via a Bluetooth enabled printer. 
Follow these steps to connect to a Bluetooth enabled printer:
1) Press "Backspace-3-4-5-6" to turn on Bluetooth.
2) Execute "Bluetooth" Manager from the "Program" menu.
3) The Braille Sense U2 scans for Bluetooth devices. 
4) Press "Space-1" or "Space-4" to navigate to the Bluetooth enabled printer in the Bluetooth Devices List.
5) Press "Enter".
6) The Braille Sense U2 scans for available services.
7) PRESS "Space-1" or "Space-4" to navigate to the "Printer" service.
8) Press "Enter" 
9) The printer should connect to Braille Sense U2.

13.2.8 Using Multiple Services 

You can use the LAN, FTP, and ActiveSync Bluetooth services simultaneously. However, if you plan to use any of these services at the same time, you should connect the FTP service before connecting the LAN and ActiveSync services. If you do not connect the FTP service first, you may experience problems. If you are using the Serial 
Port service, you should not connect to any other Bluetooth services.

13.3 Hot keys in Bluetooth Manager

Scan for Bluetooth devices: Enter-r (dots 1-2-3-5)
Connect to device: Enter on the device name
Connect to service: Enter on the service name
Disconnect service in Bluetooth service list: Enter-d (dots 1-4-5)
Move to Bluetooth device list from service list: Backspace
Delete pairing information in Bluetooth device list: Space-d (dots 1-4-5) 

1) FTP service
Open local folder/open remote folder: Enter-o (dots 1-3-5)
Copy: Enter-c (dots 1-4)
Paste: Enter-v (dots 1-2-3-6)
Send to: Enter-s (dots 2-3-4)
Retrieve file: Enter-r (dots 1-2-3-5)
New folder: Enter-f (dots 1-2-4)
Delete file/folder: Space-d (dots 1-4-5)
Information: Enter-i (dots 2-4)